**Customer Conduit & Cable Extension Agreement**

# Ethernet Conduit Requirements:

Frontier build pricing is structured to the existing minimum point of entry (“MPOE”) /Demarc or the Right Of Way at the edge of Customer’s property; if the MPOE/Demarc (more, specifically the required facilities) do not exist, Customer shall be responsible, at its own expense, to provide conduit into the property for cable placement. The conduit should be empty of cables that have working circuits on them except when using mechanical separation such as Sub Duct.

# Ethernet Cable Extensions:

Frontier does NOT cover or provide demarc extensions, we deliver to existing demarc/MPOE only. Customer must extend from there if needed and should review this at their site to determine where this is and what their cost will be. This is especially critical in multi-tenant buildings. Their circuit hand off selection may be impacted based on the distance from MPOE to where the customers equipment is. We offer Copper RJ45, Multimode Fiber (850nm) and Single Mode Fiber (1310nm). See graphic below for details.

**Road**

Office

**Customer Provided Demarc Extension Cable**

Office

IT Closet

Office

Conference room

Cublicles

Office

**Customer Building**

Door

**Customer**

**Equipment**

**Customer Provided Conduit**

Building MPOE

**Frontier Cable**

**Frontier NID**

The cable needed for this extension must be provided/installed by the customer.

The path/conduit from the edge of the property to the MPOE must be provided by the customer. Frontier will not physically build into or on customer property.

**\*\*Moving the Frontier NID from the MPOE is not supported. To do so requires and ICB request and is considered creating a NEW MPOE and standard pricing does not apply.**

**Property Edge Outline**

**Right of Way**

# Circuit Delivery Medium:

Ethernet circuits 50M and below may be delivered to the site on copper or fiber facilities. The specific delivery medium will be determined by local Engineering post sale. The local team will also cover any site specifics with the customer contact during a post-sale site walk. To have fiber delivery for your circuit guaranteed pre-sale you will need to order 100M or higher in speed.

If you need assistance in determining which option is best, please ask to be put in touch with a Channel Solutions Engineer.

**\*By signing below, I agree to applicable Terms & Conditions set forth in the FSA and Schedules.**

**Customer Signature:** {{Signer1Signature}} **Date:** {{Signer1Date}}

**Customer Name:** {{Subscriber\_Name}}

**® AGENTS.FRONTIER.COM**

V1.0\_1-11-21